Коррекция неустойчивости киноизображений методами цифровой обработки

К.О. Гусев, Д.М. Поздеев, аспиранты 
Руководитель А.Ф. Перегудов, к.т.н.,
СПбГУКиТ
Аннотация
В статье рассматривается возможность коррекции неустойчивости киноизображений путём обработки файлов, включающих в себя собственно кинокадр и сопутствующие ему перфорации. Даётся обзор существующих программных продуктов стабилизации изображений и формируются требования к специализированному программному обеспечению для работы в составе фильм-сканера. Предлагается один из возможных алгоритмов такого программного обеспечения. 
Ключевые слова: кинокадр, неустойчивость, стабилизация, вектор движения. 

Motion Pictures Unsteadiness Correction Using Digital Processing
Kirill Gusev, Alexander Peregudov,
St.Petersburg State University of Film and Television

Abstract
In the article possibility of unsteadiness correction of scanned film frames with perforations is shown. Available software products for image stabilization are analyzed and demands are advanced for specialized image processing software working in film-scanner structure. One of possible algorithms of such a software is suggested.
Keywords: frame, unsteadiness, stabilization, motion vector.

ЛИТЕРАТУРА
1.	Перегудов А.Ф. Фильм-сканеры: между прошлым и будущим // Техника и технология кино, 2007, №5, с. 56-63.
2.	Мелик-Степанян А.М., Проворнов С.М. Детали и механизмы киноаппаратуры. Л.: Изд. ЛИКИ, 1980, с. 520. 
3.	http://www.virtualdub.org/
4.	http://www.guthspot.se/video/deshaker.htm
5.	http://www.adobe.com/products/aftereffects/
6.	http://www.apple.com/shake/
7.	SMPTE 139-2003. SMPTE standard for Motion-Picture Film (35-mm) – Perforated KS
8.	http://matlab.exponenta.ru/imageprocess/book3/11/fspecial.php
9.	Wikipedia: Edge Detection. http://en.wikipedia.org/wiki/Edge_detection