Спектроколориметр для контроля качества 
проецируемого изображения

В.В. Антонов, О.В. Круглов
Руководитель – д.т.н., профессор В.Н. Кузьмин,
ООО «НТП «ТКА»

Аннотация
В статье рассмотрены требования, предъявляемые к качеству изображения, проецируемого на экран кинозала аналоговым или цифровым кинопроекторами; 
представлен новый прибор, разработанный специалистами фирмы ООО «НТП «ТКА» на основе спектрофотометрического метода для определения яркости и координат цвета киноэкрана. Проведено сравнение характеристик прибора с зарубежными 
аналогами.
Ключевые слова: спецификация цифрового кино (DCSS), спектроколориметр, 
координаты цвета, яркость.

SPEKTROKOLORIMETER FOR QUALITY CONTROL The 
projected image

Vladimir Antonov, Oleg Kruglov
Supervisor - Vladimir Kuzmin, Dr. (Tech.), Professor

Abstract
The article describes the requirements for the quality of the image projected on the cinema screen, analog or digital cinema projector, presented a new device, developed by experts of the company TKA SCIENTIFIC INSTRUMENTS, based on the spectrophotometric method for determining the brightness and color coordinates of a movie screen, also foreseeing a comparison of characteristics device with foreign counterparts.
Keywords: specification of digital cinema (DCSS), spektrokolorimeter, coordinate colors, brightness.
       Литература
1.	ОСТ 19-155-2000. Название
Digital Cinema Initiatives, LLC, Digital Cinema System Specification Version 1.2 March 07, 2008.
http://www.jeti.com
http://www.konicaminolta.com
http://www.xrite.com
        6.  Черниловская Г. З. Об истинном угле фотометрирования «точечного» яркомера. ТКТ, 1971, №8, с. 23–27.

», 1958.