L. Tikhonova, *at\_kte@mail.ru*

System engineering modeling of the broadcasting path with frequency pre-emphasis.

Part 1: Prerequisites for modeling and device description 15

***Abstract***

 ***The first part of the article is devoted to the analysis of the prerequisites for modeling a noise reduction system used in broadcasting and based on introducing frequency predistortions into the spectrum of the transmitted signal with their subsequent exclusion on the receiving side in order to reduce the influence of high-frequency channel interference on sound quality. A scheme of a device simulating a two-channel broadcasting path with frequency predistortions at the level of functional blocks is proposed, a detailed description of the operation of the device is given.***

***References***

***1. Tikhonova L.S. System engineering modeling of the power amplifier of audio signals [Text]. – M.: World of Technique Cinema (WTC), 2014-3(8), p. 9-13.***

***2. Zlatin I.L. SystemView 6.0 - system design of electronic devices [Text]. – M.: “Hot line - Telecom”, 2006. – 424 p.***

***3. Electroacoustics and sound broadcasting: textbook for universities / I.A. Aldoshina, E.I. Vologdin, A.P. Efimov et al.; Ed. Yu.A. Kovalgin [Text]. – M.: Hot line – Telecom, Radio and communications, 2007. – 872 p. (p. 380-383, fig. 11.30).***

***4. RF patent for the invention No. 2 559821 (RU 2 559 821 C1). IPC G11B 20/24 (2006.01). A device for simulating a noise reduction system with frequency pre-emphasis [Text] / Tikhonova LS, Rastriga SN; Applicant and patent holder St. Petersburg State University of Cinema and Television. – No. 2014141188 dated 10/13/2014. Publ. 08/10/2015, bull. Number 22.***

***5. RF patent for utility model No. 184 643 (RU 184643 U1). IPC G11B 20/24 (2018.08). Squelch model [Text] / Tikhonova L.S., Rastriga S.N.; Applicant and patent holder St. Petersburg State Institute of Cinema and Television. – No. 2018111353 dated 03/29/2018. Publ. 11/01/2018, bull. Number 31***.